You are here: CSP Developer’s Guide: Overview > 7 Configuring and Using Resources on the DSP Series 2 Cards > Administration API Messages

Administration API Messages

Feature Description

See Administration.

API Messages

The following messages are used for queries and alarms.

Queries | Generic Card Query 0x0123 | Use this message to query the configuration of the DSP Series 2 card for NFS, alarms, statistics, and card-level defaults.
Statistics Query 0x0121 | Use this message to query cache and function usage statistics on the DSP Series 2 card.
System Configuration Query | Use this message to query various configuration settings in the CSP, including the following for DSP: • 0x04 - Active Conference IDs • 0x07 - Resource Threshold • 0x09 - Resource Usage Reporting • 0x10 - Detailed Conference Information • 0x11 - DSP Resource Threshold • 0x13 - Conference Speakers • 0x14 - Conferencing Features • 0x15 Child Conference Information • 0x16 Child Conference IDs
System Resource Usage Query | Use this message to query the following conferencing resource utilization information: - Timeslots in use - Timeslots available - Percent used
| Generic Report | This message is generated in response to the following DSP Query Types sent in the System Configuration Query message: • 0x04 - Active Conference IDs • 0x0A - Resource Usage • 0x10 - Detailed Conference Information • 0x13 - Conference Speakers • 0x14 - Conferencing Features • 0x15 - Child Conference Information • 0x16 - Child Conference IDs
| Tone Query 0x005A | Use this message to query the transmit and receive tones assigned to a DSP, as well as the frequency and power levels of the tones.
| Call Progress Analysis Configuration Query 0x008A | Use this message to query call progress analysis (CPA) configuration information.
| Transmit Cadence Pattern Query 0x0059 | Use this message to query any of the configured transmit cadence parameters.
| Card Status Query 0x0083 | Use this message to query the number of DSP modules and their function types configured on the DSP Series 2 cards. You can address the Card Status Query message to the I/O slot behind the DSP Series 2 cards. The following are possible results: • If the Multi-Function Media I/O card is present, the Card Type contains 0xCA. • If the Multi-Function Media I/O Plus card is present, the Card Type contains 0x92. • If an illegal I/O card is present the Card Type is 0xAA. • If no I/O card is present the CSP nacked the message with status 0x61-Invalid Slot
General | Alarm 0x00B9 | This message is sent by the CSP to indicate alarm conditions on the DSP Series 2 card. See DSP Alarms in the DSP Series 2 Card Product Description chapter for more information.
Card Status Report 0x00A6 | This message is sent by the CSP platform to report the number of DSP modules and their function types configured on the DSP card.

Digital Signal Processor
Pattern of tones and silence, such as a busy signal.