0x01D1 RTP Payload Redundancy

Use this TLV to set the redundancy packet depth for RTP at configuration time. You can also set the RTP packet depth in real time, using an Outseize Control or Route Control message.

Used in:
0x1E Generic PPL ICB in:
Resource Attribute Query message
Resource Attribute Configure message

Byte | Description
0, 1 | Tag: 0x01D1 RTP Payload Redundancy
2, 3 | Length: 0x0001
4 | Value[0] 0x00 No Redundancy (Default) 0x01 Redundancy Level 1 (Not supported by Profile 4 on the IPN-3 card.)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.
Outgoing call setup during real-time call processing on a specific channel.
See Programmable Protocol Language.
See Information Control Block.