L3P Call Control PPL Timers (0x0005)

When specifying new timer values, remember that all PPL Timers are specified in 10 ms increments. For example, a PPL timer for 4 seconds is specified as 4000 (decimal, 400 x 10 ms = 4 seconds), which is the hexadecimal value of (0x190).

Timer ID | Description | Value (default)
--- | --- | ---
0x01 | Outseize Response Wait | 60 seconds (6000 10ms units)
0x02 | Register Request Wait | 8 seconds
For Euro-ISDN only
0x02 | INFO message wait for Overlap Receive | 20 seconds
0x03 | INFO message wait for Overlap Send | 20 seconds
0x04 | Register Request Wait | 8 seconds

See Programmable Protocol Language.
Outgoing call setup during real-time call processing on a specific channel.
See Integrated Services Digital Network.