You are here: CSP Hardware Product Descriptions > 6 Resource Cards > Dialogic® Digital Signal Processing Series One Card - See Model Numbers

Dialogic® Digital Signal Processing Series One Card - See Model Numbers

Description

The Dialogic® Digital Signal Processing Series One Card inserts a group of powerful DSPs into the Pulse Code Modulation (PCM) data path. Each DSP-ONE can provide the services of 22 Dual Tone Multi-Frequency (DTMF) receivers, permitting one DSP-ONE card to carry 352 DTMF receivers. You can populate each DSP-ONE card with up to 16 DSPs.

The DSPs are mounted on modules referred to as logical SIMMs, with up to eight DSPs per SIMM. Up to two SIMMs can be mounted on the DSP-ONE card, for a total of 16 DSPs per DSP-ONE card.

Function

The DSP-ONE card can perform a single function or many of the following functions:

• Tone generation

• Tone detection

• Conferencing

• Voice recorded announcements

• Signal energy detection

• Dial pulse detection

Battery

The card has 4 MB of battery-backed RAM.

Placement

The DSP-ONE card resides in the front slot of a CSP 2090,
CSP 2110 or CSP 2040 chassis.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the board.

Specifications

The DSP-ONE card is designed to the following electrical, physical and environmental specifications

Electrical | Specification
--- | ---
Supply Voltage, Vcc | 5.00V
Supply Current, Vcc @ 5.0V | 7.6A (typical)

Physical | Specification
--- | ---
Height | 9.3 inches (236.2 mm)
Depth | 12.5 inches (317.5 mm)
Width | .775 inches (19.7 mm)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

DSP-ONE Card Models

The available DSP-ONE card models are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
DSP-ONE with (1) C31-8 Module | CSP-DSP-1102 | CSP-DSP-1102R
DSP-ONE with (2) C31-8 Modules | CSP-DSP-1202 | CSP-DSP-1202R
DSP-ONE with (1) C31-8 and (1) C31-VRA Module | CSP-DSP-1112 | CSP-DSP-1112R
DSP-ONE with (1) C31-VRA Module | CSP-DSP-1012 | CSP-DSP-1012R
DSP-ONE with (2) C31-VRA Modules | CSP-DSP-1022 | CSP-DSP-1022R

Related Products

The products related to the DSP-ONE card are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
Not Applicable | Not Applicable | Not Applicable

Front and Side Views

The front and side views show the LEDs, push button switches, Monitor connector, DIP switches, and jumpers.

Controls and Indicators

The table below describes the LEDs and push button switches as shown in the front view of the DSP-ONE Card.

LEDs | Color/Status | Description
--- | --- | ---
Status | Red | The Stop push button has been pressed. The card is disconnected from the system buses.
Green | The card is connected to the system buses.
Off | The card is resetting.
Halt | Red | The CPU has halted. This LED is red briefly during card reset.
Green | The CPU is running.
Diag | Green | This LED is green except during a card reset when this LED goes out briefly.
Amber | This LED is amber during diagnostic tests.
Push Buttons | Description
Stop push button | Removes card from the system buses. Always press the Stop push button before removing the card from the chassis.
Reset push button | Initiates CPU reset on the card. The software configuration is maintained.

DIP Switch S1

The table below describes the DIP switch S1 settings. The shading (asterisk* for html documents) indicates factory-installed settings.

Position | Setting | Function
--- | --- | ---
1 | ON* | Disables Debug 1 Mode
OFF | Enables Debug 1 Mode (printing)
2 | ON* | Selects 9600 baud for Monitor port
OFF | Selects 19200 baud for Monitor port
3 | ON* | Disables Debug 2 Mode
OFF | Enables Debug 2 Mode
4 | ON* | Reserved, normally should be ON
OFF | Reserved
5 | ON* | Reserved, normally should be ON
OFF | Reserved
6 | ON* | Reserved, normally should be ON
OFF | Reserved
7 | ON* | Reserved, normally should be ON
OFF | Reserved
8 | ON* | Reserved, normally should be ON
OFF | Reserved

Jumpers

The table below indicates the jumper settings.

Jumper | Setting | Description
--- | --- | ---
JP1 | Not Installed (default) | Factory use only
JP2 | Not Installed (default) | Factory use only
JP3 | Not Installed (default) | Factory use only
JP4 | Installed (default) | Enables battery backup
JP5 | Installed (default) | Factory use only
JP6 | Installed (default) | Factory use only

PCM. Common technique of encoding analog voice into a digital bit stream where samples are taken 8000 times per second.
See Pulse Code Modulation.
Digital Signal Processor
Random Access Memory