You are here: PPL Developer’s Guide > 6 SS7 Atomic Functions > ISUP BLS, HGBS MGBS

ISUP BLS, HGBS MGBS

The following atomic function is used by the following components:

• ISUP BLS (0x0016)

• ISUP HGBS (0x007)

• ISUP MGBS (0x0045)

AF Number | 69
--- | ---
Name | Check ISUP variant ID
Description | Finds ISUP variant ID of the stack.
Arg1 | <Not Used>
Arg2 | <Not Used>
Result | Returns a PPL event corresponding to the variant ID configured.

See Integrated Services Digital Network User Part.
See Atomic Function.
See Programmable Protocol Language.
In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.