L3P Call Control PPL Events

Event Number | Event Name
--- | ---
0x50 | L4 Call Request
0x51 | L4 Alerting Request
0x52 | L4 Connect Request
0x53 | L4 Internal Connect Request
0x54 | L4 Clear Request
0x55 | L4 Inseize Control
0x56 | L4 Outseize Control
0x57 | L4 Purge
0x64 | L3 SETUP Indication
0x65 | L3 INFORMATION Indication
0x66 | L3 CALL PROCEEDING Indication
0x67 | L3 ALERTING Indication
0x68 | L3 PROGRESS Indication
0x69 | L3 CONNECT Indication
0x6A | L3 USER INFORMATION Indication
0x6B | L3 DISCONNECT Indication
0x6C | L3 Clear Indication
0x6D | L3 Error Indication
0x6E | L3 FACILITY Indication
0x6F | L3 FACILITY ACK Indication
0x70 | L3 FACILITY REJ Indication
0x71 | L3 Facility Req Ack Indication
0x72 | L3 NOTIFY Indication
0x79 | L3 REGISTER Indication
0x7A | L3 MORE INFO Indication
0x7B | L3 RELEASE Indication
0x96 | L3_GEN_EVENT_IND_0
0x97 | L3_GEN_EVENT_IND_1
0x98 | L3_GEN_EVENT_IND_2
0x99 | L3_GEN_EVENT_IND_3
0x9A | L3_GEN_EVENT_IND_4
0x9B | L3_GEN_EVENT_IND_5
0x9C | L3_GEN_EVENT_IND_6
0x9D | L3_GEN_EVENT_IND_7
0x9E | L3_GEN_EVENT_IND_8
0x9F | L3_GEN_EVENT_IND_9

Outgoing call setup during real-time call processing on a specific channel.
Positive acknowledgment to a message