0x64 Global Object Type

The Global Object Type Address Element defines an object type such as a channel, span, or link. The object type list is common to all objects so no two objects in the system should have the same object type.

Byte | Address Element Field Description
--- | ---
0 | Address Element: 0x64
1 | Data Length: 0x02
2, 3 | Data[0,1] 0x1000 - SS7 Signaling 0x1001 - SS7 Stack 0x1020 - M3UA 0x1021 - Stack Parameter 0x1022 - Local Application Server 0x1023 - Remote Application Server 0x1024 - Local Application Server Process 0x1025 - Remote Application Server Process 0x1026 - Local Signaling Gateway 0x1027 - Remote Signaling Gateway 0x1028 - Local Signaling Gateway Process 0x1029 - Remote Signaling Gateway Process 0x102A - Route Set 0x102B - Connection

The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.
See Signaling System Number Seven.
A device that translates calls between an IP network and another network, typically the PSTN.