You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > IP Signaling Series 3 Card Query 0x0101

IP Signaling Series 3 Card Query 0x0101

SwitchKit Name

IPCallServerQuery

Type

EXS API and SwitchKit API message

Description

IP Signaling Series 3 Card Query 0x0101

This message is used by the host to query the details of the configuration data and the status of the IP Signaling Series 3 card interface.

Message Type

Configuration Query

Sent By

Host

EXS Hex API Format

Message (White) | Response (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame, (0xFE)
1, 2 | Length (0x0013) | 1, 2 | Length (0xNNNN)
3, 4 | Message Type (0x0101) | 3, 4 | Message Type (0x0101)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Sequence Number (same as message)
7 | Logical Node ID (0xFE) | 7 | Logical Node ID (0xFE)
8, 9 | Status MSB, LSB
: | AIB Address Method 0x00 - Individual AEs | : | AIB Same as message
Number of AEs to follow
AEs 0x48 Ring Communication Link 0x53 Object Type
: | Query Type 0x01 Query List of IP Signaling Series 3 Cards Configured The query response message returns a list of configured IP Signaling Series 3 cards using the Add Call Server TLV. | : | Number of TLVs to Follow
: | 0x02 Query Basic Information | : | TLVs 0x0005 IP Signaling Series 3 Card Slot Number 0x0007 Reserved 0x0008 IP Signaling Series 3 Card Compatibility Tag 0x000A Add Poll Interval 0x000C Matrix IP Address 0x000E IP Signaling Series 3 Card Interface Service State 0x000F Link Down Timer
: | Reserved (0x00) |  |
: | Checksum | : | Checksum

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
Most Significant Bit
Least Significant Bit
See Address Information Block.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.