0x05E9 Initial Silence Timer

Use this TLV in the Record File Start message to set the Initial Silence Timer.

Recording does not begin until voice is detected. If the Initial Silence Timer expires before voice is detected, the recording attempt is aborted. For example, if the default setting of 2500 milliseconds is used, the recording attempt is aborted if no voice is detected in the first 2500 milliseconds.

Byte | Description
0, 1 | Tag 0x05E9 Initial Silence Timer
2, 3 | Length 0x0002
4, 5 | Value[0-1] Timer (10 ms increments) Minimum 1 (0x0001) Maximum 65534 (0xFFFE) Disable timer 65535 (0xFFFF) Default 250 (0x00FA)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.