0x000F IP Signaling Series 3 Card Interface Support

Used in:
IP Signaling Series 3 Card Configure message (0x0100)

Byte | Description
--- | ---
0, 1 | Tag 0x000F
2, 3 | Length 0x0010
4 | Value[0] L3/L4 Signaling Interface, MSB 0x00
5 | Value[1] L3/L4 Signaling Interface, LSB 0x00 Disable 0x01 Enable
6 | Value[2] LX/ENG Connection Interface, MSB 0x00
7 | Value[3] LX/ENG Connection Interface, LSB 0x00 Disable 0x01 Enable
8-20 | Value[4-16] Reserved 0x00 (Disabled)

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Most Significant Bit
Least Significant Bit