You are here: CSP Hardware Product Descriptions > 4 Common Channel Signaling Cards > CCS I/O Series 3 Red Cable - Part Nos. 64333300/164333300

CCS I/O Series 3 Red Cable - Part Nos. 64-3333-00/164-3333-00

Description

The CCS I/O Series 3 Redundancy Link cable assembly serves as an independent link for redundancy between the adjacent CCS I/O Series 3 cards using the Redundant Link connectors.

Specifications

The Redundancy Link cable is designed to the following specifications.

Parameter | Specification
--- | ---
Length | 7 inches
Connector Types | 8-Pin, RJ-45 connectors

Related Products

The products related to the Redundancy Link cable are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
CCS I/O Series 3 Card | EXS-7IO-1300 | EXS-7IO-1300R

Assembly Diagram and Pinouts

The Redundancy Link cable assembly and pinouts are shown below.

DASS2/DPNSS Card - EXS-DAS-1000

The DASS2/DPNSS card is no longer supported in the CSP.

See Common Channel Signaling.