You are here: CSP API Reference > 3 Information Control Blocks > SS7 and ISDN Values > Information Elements

Information Elements

Formatted IEs with Event include IE data fields. The data included in the format depends on the IE type. The data fields for each IE type is listed below. For more information on IE field values, refer to the CSP Developer’s Guide: Common Channel Signaling.

CCS. Network architecture using SS7 protocol for the exchange of information between telecommunications nodes and networks on an out-of-band basis.