You are here: CSP Developer’s Guide: Common Channel Signaling > 7 SS7 PPL Information > ISUP CGRS (0x001B)

ISUP CGRS (0x001B)

Purpose

This section includes PPL Config Bytes for the PPL Component ISUP CGRS.

ISUP CGRS Configuration Bytes

Byte | Description | Value
--- | --- | ---
0x01 | This config byte determines the number of retries of GRS that will be sent to the network when an unequipped CIC (UCIC) is received in a response. The circuit group reset (GRS) is retried n times or until a circuit group reset acknowledgment GRA is received (whichever is earlier). | 0x00 (default) The valid range is 0-255.

See Programmable Protocol Language.
A programmable software component that uses PPL state machines that can be modified with the PPL Tool.
See Integrated Services Digital Network User Part.
See Circuit Identification Codes.