0x000C Matrix IP Address

Used in:
IP Signaling Series 3 Card Configure message (0x0100)
IP Signaling Series 3 Card Query message (0x0101)

Byte | Description
0, 1 | Tag 0x000C
2, 3 | Length 0x0006
4-7 | Value[0-3] IP Address (4 Bytes)
8, 9 | Value[4, 5] Port Number

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."