0x0035 LAPD Status

Used in:
PPL Event Request message
PPL Event Indications message

ICB Type | 0x03 (Extended Data)
ICB ID | 0x0035
Data Length | 0x0001
LAPD State | Variable

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.
Link Access Protocol (Procedure) – D channel (ISDN)
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.