You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Answer Supervision Mode Configure 0x00BB

Answer Supervision Mode Configure 0x00BB

SwitchKit Name

AnswerSuperviseConfig

Type

EXS API and SwitchKit API message

Description

Answer Supervision Mode Configure 0x00BB

Use this message to configure the Answer Supervision mode for a channel or range of channels.

The Answer Supervision Mode options are:

Propagate Answer to Distant End

Notify Host of Answer

Propagate Answer to Distant End and Notify Host of Answer

No Answer Supervision - no propagation of answer or notification

Do not send this message for channels configured as the following trunk types: DP0 DPT FX0 loopstart and groundstart (OK to use if the answer supervision mode is 0x00 or 0x03) If you use this message for these trunk types, the CSP sends the response Status value "Invalid Data Type" (0x17).

Sent by

Host

Example Message
(SwitchKit Socket Log Output)

The following socket log output/example message configures the Answer Supervision Mode to propagate answer to distant end for channels 0x00 - 0x17 on spans 0x01 - 0x02.

00 12 00 BB 00 00 FF 01 02 0D 03 00 01 00 0D 03 00 02 17 00

SwitchKit Code

Configuration

AnswerSuperviseConfig (

Node = integer,

Range = StartSpan : StartChan - EndSpan : EndChan,

AnswerMode = integer);

C Structure

typedef struct {

unsigned short StartSpan;

UBYTE StartChannel;

unsigned short EndSpan;

UBYTE EndChannel;

UBYTE AnswerMode;

} XL_AnswerSuperviseConfig;

C++ Class

class XLC_AnswerSuperviseConfig : public XLC_ChanRangeMessage {

public:

unsigned short getStartSpan() const;

void setStartSpan(unsigned short x);

UBYTE getStartChannel() const;

void setStartChannel(UBYTE x);

unsigned short getEndSpan() const;

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x00BB) | 3, 4 | Message Type (0x00BB)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x01 - Range | 8, 9 | Status MSB, LSB
Number AEs to follow
AEs
| 0x0D Channel (Starting) 0x0D Channel (Ending) | 10 | Checksum
: | Answer Supervision Mode Enter one of the following values: 0x00 Propagate Answer to Distant End (default) 0x01 Notify Host of Answer 0x02 Propagate Answer to Distant End and Notify Host of Answer 0x03 No Answer Supervision No propagation of answer or notification FX0 Loopstart/FX0 Groundstart The only valid entries for FX0 loopstart and FX0 groundstart are 0x0000 and 0x0003.
: | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit