0x52 IP Signaling Series 3 Card ID or Expanded Logical Node ID

This AIB is generic. It can be used in any of the newer (introduced in 8.0 and above) Configure and Query messages for any component. If you use this AIB in the IP Signaling Series 3 Card Configure message (0x0100) you must also use AIB 0x53.

Byte | AIB Field Description
--- | ---
2 | Address Element: 0x52
3 | Data Length: 0x02
4 | Data[0, 1] Expanded Logical Node ID This field addresses the node/IP Signaling Series 3 Card ID and is used by the host application to route the messages to the proper node/ IP Signaling Series 3 Card. Logical Node ID in the header is ignored (it is set to 0xFE) and Expanded Logical Node ID is used to address the node.

See Address Information Block.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.