0x000C V5 Add Link

Used in:
V5 Configure message
V5 Configuration Query message

Byte | Description
0 | Tag 0x00 V5 Add Link (MSB)
1 | Tag 0x0C V5 Add Link (LSB)
2 | Length 0x00 (MSB)
3 | Length 0x04 (LSB)
4 | Logical Span ID for Link, MSB 0x00
5 | Logical Span ID for Link, LSB 0x00
6 | V5 Link ID (0 - 15) 0x00
7 | Real V5 Link ID (0 - 255) 0x00

Most Significant Bit
Least Significant Bit
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.