E1/T1

Comp. ID | Comp. Name | PPL Assign | PPL Audit Config | PPL Audit Query | PPL Config | PPL Data Query | PPL Event Request | PPL Timer Config
--- | --- | --- | --- | --- | --- | --- | --- | ---
0x0001/0x0003 | E1/T1 | Channel (0x0D)

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)