# 2 VDAC-ONE Card

This chapter provides information you need to configure the
VDAC-ONE (Voice-Data Access Concentrator) card.

In this section:

VDAC-ONE Card Overview

Basic Configuration

IP Resources Attributes

General IP Attributes

Voice Attributes

Jitter Buffer Delay/Adaptation Rate

Fax Attributes

IP Connection Management

Dynamic Connection Management

Release Mode Configuration

Loopback for Testing

Routing Examples

Sample Route Control / Resource Attribute Configure

VDAC VoIP - 0x009C