You are here: CSP Developer’s Guide: Line Cards > 2 T1 Information > Default Instruction Lists

Default Instruction Lists

Default Inseize Instruction List

The default inseize instruction lists for T1 spans are shown in the table below.

Channel | Instruction List
--- | ---
T1 | 1. Report Incoming Call 2. Wait For Host Control

Default Outseize Instruction Lists

The default outseize instruction lists for T1 spans are shown in the table below.

Channel | Instruction List
--- | ---
T1 | 1. Wait For Host Control Message

Configuring Instruction Lists

You must send a separate message for each instruction you add to the list. For example, to configure the following inseize instruction list on all of the channels on Span 0, send the following sequence of Inseize Instruction List Configure messages, with the specifications noted:

Instruction List

1. Generate Wink 1

2. Receive Stage 1 Digits

3. Report Incoming Call with Address Data

4. Wait for Host Control

Send the following Inseize Instruction List Configure messages:

Message 1:

Instruction Number: 0x01
Instruction Type: 0x02 (Generate Call Processing Event)
Instruction Data Byte 1: 0x03 (Wink 1)

Message 2:

Instruction Number: 0x02
Instruction Type: 0x03 (Receive Stage N Address Data)
Instruction Data Byte 1: 0x01 (Stage 1)

Message 3:

Instruction Number: 0x03
Instruction Type: 0x06 (Report Incoming Call With
Address Data)

Message 4:

Instruction Number: 0x04
Instruction Type: 0x04 (Wait For Host Control)

Incoming call setup during real time call processing on a specific channel.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
Outgoing call setup during real-time call processing on a specific channel.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
Momentary interruption in a single frequency tone indicating the distant switch is ready to receive the digits just dialed.