You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Reset Matrix 0x009D

Reset Matrix 0x009D

SwitchKit Name

ResetMatrix

Type

EXS API or SwitchKit API message

Description

Reset Matrix 0x009D

This message is used by the host to force a matrix to reset. If the host sends it to the active CSP Matrix Series 3 Card in a redundant system, it will result in a CSP Matrix Series 3 Card switchover. A switchover can also be initiated by sending a Become Active message to the standby CSP Matrix Series 3 Card.

Sent by

Host

Related API Messages

Become Active 0x00A1 (ActivateMatrix)

SwitchKit Code

C Structure

typedef struct {

} XL_ResetMatrix;

C++ Class

class XLC_ResetMatrix : public XLC_OutboundMessage {

public:

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x0005) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x009D) | 3, 4 | Message Type (0x009D)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
8 | Checksum | 8, 9 | Status MSB, LSB
10 | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
Most Significant Bit
Least Significant Bit