You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Clear IP Signaling Series 3 Card 0x0108

Clear IP Signaling Series 3 Card 0x0108

Type

EXS API message

Description

Clear IP Signaling Series 3 Card 0x0108

This message clears the system software on the IP Signaling Series 3 card before and/or after the IP Signaling Series 3 card interface is established. This message is sent directly to the IP Signaling Series 3 card and uses the extended logical node ID format.

To initiate the download of the new software load, you need to reset the IP Signaling Series 3 card by pushing the Reset button or using the Reset IP Signaling Series 3 Card message (0x0107).

Sent by

Host

Example Message

The following clears the system software on the IP Signaling Series 3 card when the IP Signaling Series 3 card ID or Matrix ID is not assigned.

00 11 01 08 00 00 fe 00 02 52 02 ff ff 53 04 00 20 ff ff

Hex API Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0xNNNN)
3, 4 | Message Type (0x0108) | 3, 4 | Message Type (0x0108)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Sequence Number (same as message)
7 | Extended Logical Node ID (0xFE) | 7 | Extended Logical Node ID (0xFE)
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status MSB, LSB (0x0010)
Number of AEs to follow
AEs 0x48 Ring Communication Link 0x53 Object Type
: | Checksum | : | AIB Same as message
: | Checksum

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit