0x2946 - SIP Request URI Password

Used in:
PPL Event Request message
PPL Event Indication message

Byte | Description
0, 1 | Tag 0x2946
2, 3 | Length Variable (maximum 20 bytes)
4-n | Value[0-n] Null-terminated ASCII string

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
American Standard Code for Information Interchange