You are here: CSP Hardware Product Descriptions > 1 Chassis > Dialogic® CSP 2090 Chassis - EXS-CHA-1100/EXS-CHA-1100R

Dialogic® CSP 2090 Chassis - EXS-CHA-1100/EXS-CHA-1100R

Description

The Dialogic® CSP 2090, a mid-range chassis configuration of the Converged Services Platform (CSP) is designed to meet the demands of the telecommunication industry by delivering high performance, fault tolerant switching in a compact microprocessor-based design.

A typical CSP 2090 chassis can accommodate up to 2,048 ports, support matrix CPU cards, a fully configurable combination of line and services cards, and a host interface. The CSP supports redundancy and the cards are hot swappable. Blockout cards are required for proper air flow and cooling. Any unoccupied line card slot or I/O card slot should have a Blockout card installed.

The CSP 2090 supports common channel signaling packet engines for both ISDN and SS7 communications. Line protocol cards include E1, T1 and J1 services. Standard and custom tone generation and reception, precise call analysis, conferencing and voice recorded announcements are provided through an advanced Digital Signal Processing unit available for the CSP.

The CSP 2090 can operate as either a stand-alone unit, or as a unit in a larger system.

Features

The CSP 2090 chassis consists of the following:

• Two fan trays, front and rear

• A midplane bus, which is a high-speed communication line for connecting individual line cards and I/O cards

• A 20 card slot chassis (with dedicated CPU and power card slots)

• Mounting brackets so the chassis can be mounted in a 19" or 23" rack.

Configuration Information

The part number, serial number, model number, and revision are located on the side of the chassis.

Specifications

The CSP 2090 chassis is designed to the following electrical, physical and environmental specifications.

Electrical | Specification
--- | ---
Input Power Requirement | -48 V DC, 25A (maximum)
Input Voltage Range | -40 V DC to -60 V DC

Physical | Specification
--- | ---
Height | 39.9 cm (15.7 in.)
Width | 43.8 cm (17.25 in.)
Depth | 48.6 cm (19.125 in.)
Weight | 30 kg (65 lb.) (empty chassis with fan trays and blockout cards installed) 45 kg (100 lb.) (loaded chassis)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Front View

The front of the chassis has dedicated slots for the CSP Matrix Series 3 and Power cards. Slots 0-15 are for the other line cards.

Rear View

The rear of the chassis has dedicated slots for the CSP Matrix Series 3 I/O cards. Slots 0-15 are for the other I/O cards. The power input panel is also located at the rear of the chassis

Cross Sectional View

This shows the approximate location of the fan trays and the front and rear card cages.

An Internet Protocol enhanced service node that supports the deployment of voice and data services in circuit, packet, and converged networks. The Converged Services Platform (CSP) features an open and multi-functional platform design that enables developers to quickly create and deliver new revenue-generating services for both legacy and next-generation networks.
See Integrated Services Digital Network.
See Signaling System Number Seven.
A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)