0x01DD Flush ARP Cache Table Entry

Send this TLV to remove entries from an ARP Cache table. You must also include a VoIP Module TLV to indicate the module.

To remove all entries in the table, enter a length of 0x0000.

To remove an entry for a specific IP address, enter a length of 0x0004 and enter the IP address in Data[4-7].

To remove an entry for a specific Ethernet address, enter a length of 0x0006 and enter the Ethernet address in Data[4-9].

Used in:
ARP Cache Query

Byte | Description
0,1 | Tag Flush ARP Cache Table Entry (0x01DD)
2, 3 | Length Variable (see below)
4 | Value: 0x0000 To remove all entries on the module. There is no data. 0x0004 To remove a specific IP address. Also enter the IP address in Data[4-7]. 0x0006 To remove all entries at an Ethernet Address. Also enter the Ethernet address in Data[4-9].

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.