TUP SPRC Configuration Bytes

Byte | Description | Value
--- | --- | ---
0x01 | SIO Subservice Field | 0x08
0x02 | SIO Service Indicator | 0x04
0x0A | Pause/Resume Option | 0x00
0x0B–0x27 | Unused |
Congestion Control
0x28 | Number of probes to determine Average Delay | 10
0x29 | Probe Delay Threshold for Incoming Calls, 100 ms units | 100 ms
0x2A | Average Delay Threshold for Incoming Calls, 100 ms units | 50 ms
0x2B | Congestion Cleared Threshold for Incoming Calls, 100 ms units | 10 ms
0x2C | Number of probes to determine congestion cleared=Incoming Calls | 10
0x2D | Probe Delay Threshold for Outgoing Calls, 100 ms units | 100 ms
0x2E | Average Delay Threshold for Outgoing Calls, 100 ms units | 50 ms
0x2F | Congestion Cleared Threshold for Outgoing Calls, 100 ms units | 10 ms
0x30 | Number of probes to determine congestion cleared=Outgoing Calls | 10
0x31–0xC8 | Unused |