0x0168 VDAC Module IP Address

Use this TLV to populate the Router Component (0x0064) with the VDAC module IP address.

Used in:
PPL Table Download message

Byte | Description
0, 1 | Tag 0x0168
2, 3 | Length 0x0004
4-7 | Value[0-3] IP Address of VDAC module

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
See Programmable Protocol Language.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).