0x2928 SIP From Display Name

This TLV contains the user name parsed from the display name in ASCII format.

Used in:
0x0033 NPDI Universal ICB in:
Request for Service with Data message
Route Control message
Outseize Control message

Byte | Description
0, 1 | Tag 0x2928
2, 3 | Length Variable (Maximum of 250 bytes)
4-n | Value A Null-terminated ASCII string containing From Display Name

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
American Standard Code for Information Interchange
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Outgoing call setup during real-time call processing on a specific channel.