L3P BT IUP PPL Timers

Timer ID | Timer | Default Value | Default Duration
--- | --- | --- | ---
0x01 | TO-1 | 18000 | 180 seconds
0x02 | TO-2 Non-receipt of answer | 12000 | 120 seconds
0x03 | TO-3 | 30000 | 300 seconds
0x04 | TO-4 | 12000 | 120 seconds
0x05 | Awaiting answer | 6000 | 60 seconds
0x09 | Awaiting appropriate backward message after IFAM/IAM/SAM/FAM or Forward Group 7 message is sent during call setup phase | 2000 | 20 seconds
0x0E | Await receipt of additional Information Message | 500 | 5 seconds
0x10 | Prolonged Call Setup | 18000 | 180 seconds
0x11 | Non-receipt of SAM/FAM in response to SAD | 2000 | 20 seconds
0x12 | Non-receipt of SAM or FAM in response to Send N Digits. |  | Dynamic based on number of requested digits and Exchange Type.
0x14 | Hardware Blocking Timer | 12000 | 120 seconds
0x15 | TO-21 Call Clear Timer | 30000 | 300 seconds
0x16 | IAM-SAD maximum digit collection timer | 400 | 4 seconds --This value must be less than the value set for 0x11.
0x17 | Block Timer | 12000 | 120 seconds