0x05F0 DSP 2 Main Board Memory Alarm Threshold Configure

Use this TLV to set the threshold in percentage of total blocks used, on a per-card basis. If recorded voice files are accessed through a Network File Server, then this value represents only the Temporary Cache memory space. Files are stored in one-second blocks.

If recorded announcements are accessed through a Network File Server, then this represents only the Temporary Cache memory space.

For the DSP Series 2 card, this TLV is used in the Generic Card Configure message and in the response to the Generic Card Query message.

Byte | Description
0, 1 | Tag 0x05F0 DSP 2 Main Board Memory Alarm Threshold Configure
2, 3 | Length 0x0006
4 | Value[0] Parameter ID 0x00 Total Blocks
5 | Value[1] Disable/Enable 0x00 Disabled (default) 0x01 Enable
6-9 | Value[2-5] Threshold Value 1-100 (represents a percentage of the total available blocks)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor