0x05F1 DSP Temporary Memory Alarm Threshold Configure

Use this TLV in the Generic Card Configure message to set the threshold in percentage of total blocks, and to disable the alarm. This is set on a per-card basis, and the same threshold is used for all DSPs that are configured for File Playback/Record on that DSP Series 2 card. Files are stored in one-second blocks.

Byte | Description
0, 1 | Tag: 0x05F1- DSP Temporary Memory Alarm Threshold Configure
2, 3 | Length: 0x0006
4 | Value[0]: Parameter ID 0x00 - Total Blocks
5 | Value[1:] Disable/Enable 0x00 - Disable (default) 0x01 - Enable
6-9 | Value[2-5]: Threshold Value 1-100 (represents a percentage of the total available blocks)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor