0x0617 Alarm Threshold Query

Use this TLV in the Generic Card Query message (0x0123) to query the Alarm Threshold on the DSP Series 2 card.

Byte | Description
0, 1 | Tag: 0x0617 Alarm Threshold Query
2, 3 | Length: 0x0001
4 | Value[0]: Alarm Number Being Queried 0x00 - 0x0F 0xFF - Request a Bit Mask of Enabled Alarms

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor