0x2717 Called Party Number

Use this TLV to specify the called party number. This TLV and be used in Interworking and Standard environments.

Used in:
0x0033 NPDI Universal ICB in:
Request for Service with Data message
Route Control message

Byte | Description
0, 1 | Tag 0x2717
2, 3 | Length Variable
4 | Value[0] Type of Number
5 | Value[1] Numbering Plan Identifier and Reverse Charge Indicator
6 | Value[2] Number of Digits (N)
7 | Value[3] BCD Digit Pair 1
: | Value[4] BCD Digit Pair 2
: | Value[(N+1)/2] H alf as many BCD pairs as digits.

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Interworking is a software feature within the Excel platform call control layer that enables protocol conversion by analyzing and converting Network Signaling (NS) Layer 3 information.
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.