0x02BC Gatekeeper IP and Port

The Gatekeeper IP and Port Configure TLV is used only if the RAS module is configured during the stack configuration.

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x02BC Gatekeeper IP and Port
2, 3 | Length 0xN NNN
4 | Value[0] Configure/Deconfigure option 0x00 Configure (Default) 0x01 Deconfigure
5 | Value[1] Number of Gatekeepers. 0x01 (Default) First entry is primary Gatekeeper. The rest are alternate Gatekeepers 0xM (M = 0x01 - 0x06)
6-9 | Value[2-5] IP Address
10, 11 | Value [6-7] Port Number
: | Value [8-11] IP Address (4 Bytes)
: | Value [12-13] Port Number (2 Bytes)
: | :

An H.323 entity on the network that provides address translation and controls access to the network for H.323 terminals and other end points. The gatekeeper may also provide other services to the endpoints such as bandwidth management and locating gateways.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
The Registration, Admission, and Status messages communicated between two H.323 entities for example between an Endpoint and a Gatekeeper.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).