# 8 DSP Series 2 Cards
Product Description

DSP Series 2 Card Configurations

The CSP supports the following DSP Series 2 cards and associated I/O cards:

• DSP Series 2 and associated Multi-Function Media I/O

• DSP Series 2 Plus and associated Multi-Function Media I/O Plus

The Overview section in this chapter provides detailed information on the DSP Series 2 Plus card and a comparison to the DSP Series 2 card.

Important! In this document, unless otherwise stated, DSP Series 2 will be used for both the DSP Series 2 and DSP Series 2 Plus cards. Any software or hardware differences are indicated.

In this section:

Overview

DSP Series 2 Card

DSP Series 2 Plus Card

Features

Architecture Overview

Hardware

DSP Resource Points

Determining your DSP Resource Point Needs

DSP Resource Specifications

Mixing DSP Cards in a CSP

Default DSP Function Type Configuration

Redundancy

Ethernet Link Redundancy

Administration

Media Streaming over RTP

File Record And Playback

Overview

File Storage

Encoding Formats

VIF Format

File Retrieval Process

Playback Features

Conferencing

Overview

Unified Conference

Monitor Conference

Conferencing Features

Tones

Overview

Terms

Tone Generation

Call Setup

Energy Detection

T.30 Fax

Overview

Supported Features

Fax Applications

Administration

Overload Management

Statistics Query

Cache Query

DSP Alarms

Specifications

DSP Series 2 and DSP-ONE Cards Compared

DTMF Digit Specifications

MF Digit Specifications

Default Transmit Call Progress Tones

Default Transmit Call Progress Tone Patterns

Default Tone Patterns for CPA Detection

CPA Tone Patterns

Default CPA Tone Pattern Parameters

CPA Pattern Parameter Definitions

CPA Classes

CPA Class Parameter Definitions

Pulse Dialing Detector

Digital Signal Processor