0x0030 V5 Statistics Data

Used in:
PPL Event Indication message

ICB Type | 0x03 (Extended Data)
ICB ID Data[1, 2] | 0x0030
Data Length Data[3, 4] | (MSB, LSB), (2 Bytes)
Data[5] | Data[0]
Data[6] | Data[1]
: | :
Data[N+3] | Data[N]

The following statistics values are sent to the host in the ICB Data:

Data[0] = Query Subtype
Query Subtypes:
0x00 All Protocol Statics
0x01 V5.2 ENVELOPE Layer Statistics
0x02 V5.2 LAPV Statistics
0x03 V5.2 PSTN Statistics
0x04 V5.2 CONTROL Protocol Statistics
0x05 V5.2 BCC Protocol Statistics
0x06 V5.2 LINK Protocol Statistics
0x07 V5.2 PROTECTION Protocol Data Link Statistics
0x08 V5.2 PROTECTION Protocol Interface Statistics
0x09 V5.2 SYSTEM MANAGEMENT Statistics

Each data Variable is 4 Bytes long.
Data[1] means Data[1,2,3,4] bytes

Query Subtype 0: For All Protocols

Data for PSTN Protocol Statistics:

Data[1] Number of Establish messages transmitted

Data[5] Number of Establish ack messages transmitted

Data[9] Number of Signal messages transmitted

Data[13] Number of Signal acknowledge messages transmitted

Data[17] Number of Status messages transmitted

Data[21] Number of Status enquiry messages transmitted

Data[25] Number of Disconnect messages transmitted

Data[29] Number of Disconnect complete messages transmitted

Data[33] Number of Protocol parameter messages transmitted

Data[37] Number of Establish messages received

Data[41] Number of Establish ack messages received

Data[45] Number of Signal messages received

Data[49] Number of Signal acknowledge messages received

Data[53] Number of Status messages received

Data[57] Number of Status enquiry messages received

Data[61] Number of Disconnect messages received

Data[65] Number of Disconnect complete messages received

Data[69] Number of Protocol parameter messages received

Data[73] Total connections established so far

Data[77] Number of currently active connections

Data for Control Protocol Statistics:

Data[81] Port control transmitted

Data[85] Port control ack transmitted

Data[89] Common control transmitted

Data[93] Common control ack transmitted

Data[97] Port control received

Data[101] Port control ack received

Data[105] Common control received

Data[109] Common control ack received

Data for BCC Protocol Statistics:

Data[113] Allocation messages transmitted

Data[117] Allocation messages received

Data[121] Deallocation requests transmitted

Data[125] Decollating requests received

Data[129] Allocation rejects transmitted

Data[133] Allocation rejects received

Data[137] Allocation complete transmitted

Data[141] Allocation complete received

Data[145] Deallocation complete transmitted

Data[149] Deallocation complete received

Data[153] Audit transmitted

Data[157] Audit received

Data[161] Audit complete transmitted

Data[165] Audit complete received

Data[169] Fault transmitted

Data[173] Fault received

Data[177] Fault ack transmitted

Data[181] Fault ack received

Data[185] Protocol error transmitted

Data[189] Protocol error received

Data for LINK Protocol Statistics:

Data[193] Number of Link Control transmitted

Data[197] Number of Link Control received

Data[201] Number of Link Control Ack transmitted

Data[205] Number of Link Control Ack received

Data for PROTECTION Protocol Data Link:
(Statistics for Primary C Channel)

Data[209] Number of messages transmitted

Data[213] Number of messages received

Data for PROTECTION Protocol Data Link:
(Statistics for Secondary C Channel)

Data[217] Number of messages transmitted

Data[221] Number of messages received

Data for PROTECTION Protocol Interface Statistics:

Data[225] Number of Switchover request transmitted

Data[229] Number of Switchover request received

Data[233] Number of Switchover command transmitted

Data[237] Number of Switchover command received

Data[241] Number of Operator initiated switchover command
transmitted

Data[245] Number of Operator initiated switchover command
received

Data[249] Number of Switchover ack transmitted

Data[253] Number of Switchover ack received

Data[257] Number of Switchover reject transmitted

Data[261] Number of Switchover reject received

Data[265] Number of Reset sequence number command transmitted

Data[269] Number of Reset sequence number command received.

Data[273] Number of Reset sequence number ack transmitted

Data[277] Number of Reset sequence number ack received

Data[281] Number of Protocol error transmitted

Data[285] Number of Protocol error received

Data for SYSTEM MANAGEMENT Statistics:

Data[289] Number of times the ISDN port status T1 timer expired

Query Subtype 1: V5.2 ENVELOPE Layer Statistics:

Data[1] Number of Information frames transmitted

Data[5] Number of Information frames received

Data[9] Number of frames dropped

Query Subtype 2: V5.2 LAPV Statistics:

Data[1] Information frames transmitted

Data[5] Receive ready frames transmitted

Data[9] Receive not ready frames transmitted

Data[13] Reject frames transmitted

Data[17] Set asynchronous balanced mode frames transmitted

Data[21] Unnumbered acknowledge frames transmitted

Data[25] Disconnect mode frames transmitted

Data[29] Information frames transmitted

Data[33] Receive ready frames transmitted

Data[37] Receive not ready frames transmitted

Data[41] Reject frames received

Data[45] Set asynchronous balanced mode frames received

Data[49] Unnumbered acknowledge frames received

Data[53] Disconnect mode frames received

Data[57] Invalid frames received

Data[61] Set asynchronous balanced mode errors

Query Subtype 3: V5.2 PSTN Statistics:

Data[1] Number of Establish messages transmitted

Data[5] Number of Establish ack messages transmitted

Data[9] Number of Signal messages transmitted

Data[13] Number of Signal acknowledge messages transmitted

Data[17] Number of Status messages transmitted

Data[21] Number of Status enquiry messages transmitted

Data[25] Number of Disconnect messages transmitted

Data[29] Number of Disconnect complete messages transmitted

Data[33] Number of Protocol parameter messages transmitted

Data[37] Number of Establish messages received

Data[41] Number of Establish ack messages received

Data[45] Number of Signal messages received

Data[49] Number of Signal acknowledge messages received

Data[53] Number of Status messages received

Data[57] Number of Status enquiry messages received

Data[61] Number of Disconnect messages received

Data[65] Number of Disconnect complete messages received

Data[69] Number of Protocol parameter messages received

Data[73] Total connections established so far

Data[77] Number of currently active connections

Query Subtype 4: V5.2 CONTROL Protocol Statistics:

Data[1] Port control transmitted

Data[5] Port control ack transmitted

Data[9] Common control transmitted

Data[13] Common control ack transmitted

Data[17] Port control received

Data[21] Port control ack received

Data[25] Common control received

Data[29] Common control ack received

Query Subtype 5: V5.2 BCC Protocol Statistics:

Data[1] Allocation messages transmitted

Data[5] Allocation messages received

Data[9] Deallocation requests transmitted

Data[13] Decollating requests received

Data[17] Allocation rejects transmitted

Data[21] Allocation rejects received

Data[25] Allocation complete transmitted.

Data[29] Allocation complete received

Data[33] Deallocation complete transmitted

Data[37] Deallocation complete received

Data[41] Audit transmitted

Data[45] Audit received

Data[49] Audit complete transmitted

Data[53] Audit complete received

Data[57] Fault transmitted

Data[61] Fault received

Data[65] Fault ack transmitted

Data[69] Fault ack received

Data[73] Protocol error transmitted

Data[77] Protocol error received

Query Subtype 6: V5.2 LINK protocol Statistics:

Data[1] Number of Link Control transmitted

Data[5] Number of Link Control received

Data[9] Number of Link Control Ack transmitted

Data[13] Number of Link Control Ack received

Query Subtype 7: V5.2 PROTECTION Protocol Datalink
Statistics:

Data[1] Number of messages transmitted

Data[5] Number of messages received

Query Subtype 8: V5.2 PROTECTION Protocol Interface:

Data[1] Number of Switchover request transmitted

Data[5] Number of Switchover request received

Data[9] Number of Switchover command transmitted

Data[13] Number of Switchover command received

Data[17] Number of Operator initiated switchover command
transmitted

Data[21] Number of Operator initiated switchover command
received

Data[25] Number of Switchover ack transmitted

Data[29] Number of Switchover ack received

Data[33] Number of Switchover reject transmitted

Data[37] Number of Switchover reject received

Data[41] Number of Reset sequence number command transmitted

Data[45] Number of Reset sequence number command received

Data[49] Number of Reset sequence number ack transmitted

Data[53] Number of Reset sequence number ack received

Data[57] Number of Protocol error transmitted

Data[61] Number of Protocol error received

Query Subtype 9: V5.2 SYSTEM MANAGEMENT Statistics:

Data[1] Number of times the ISDN port status T1 timer expired

See Programmable Protocol Language.
See Information Control Block.
Most Significant Bit
Least Significant Bit
Public Switched Telephone Network
Connection between nodes, physical connectivity
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
See Integrated Services Digital Network.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)