0x275B Generic Command Response
(Interworking Only)

Use this TLV to respond to generic command. The response code should be same as the command code to confirm the command (though not required).

Used in:
0x0033 NPDI Universal ICB

Byte | Description
0, 1 | Tag 0x275B
2, 3 | Length Variable
4, 5 | Value[0,1] Generic Command Response Length MSB, LSB
6, 7 | Value[2,3] Generic Command Response MSB, LSB
: | :
: | Value[n] Generic Command Response MSB, LSB

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Most Significant Bit
Least Significant Bit