0x02 Server Socket Register by IP

Used in:
IP Socket Configure message

Byte | Description
0 | Tag 0x02 Server Socket Register by IP
1 | Length 0x0E
2 | Value[0] (0x00) Module (0xFF = base board)
3 | Value[1] Socket ID
4-7 | Value[2-5] Local IP Address (4 bytes)
8, 9 | Value[6, 7] Local Port
10-13 | Value[8-11] Remote IP Address (4 bytes)
14, 15 | Value[12, 13] Remote Port

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."