0x0687 - Enable RTP for Play/Record File

Use this TLV to enable RTP for Play/Record File in the following messages:

• Play File Start

• Record File Start

Byte | Description
0, 1 | Tag: 0x0687 - Enable RTP for Play/Record File
2, 3 | Length: 0x0001
4 | Value [0] 0x00 - Disable 0x01 - Enable

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.