0x02C0 Terminal Type

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x02C0 Terminal Type
2, 3 | Length 0x0002
4 | Value[0] 0x00 (Default) Terminal Type (MSB)
5 | Value[1] Terminal Type (LSB) 0x3C GW with no MC (Default) 0x50** GW with MC but no MP 0x5A** GW with MC and Data MP 0x64** GW containing MC w/data & audio 0x6E** GW containing MC w/data, audio, & video **Not supported in this release.

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Most Significant Bit
Least Significant Bit