You are here: CSP Hardware Product Descriptions > 2 Dialogic® CSP Matrix Controller Series 3 Cards > Debug Cable Assembly - Part Nos. 64-0046-00/164-0046-00

Debug Cable Assembly - Part Nos. 64-0046-00/164-0046-00

Description

The debug cable is connected between the Monitor port on the CSP Matrix Controller Series 3 Card and the host to set the IP address. Also set DIP S1 Positions 1 and 3 to OFF on these cards when using the debug cable.

Specifications

The debug cable assembly is designed to the following specifications.

Parameter | Specification
--- | ---
Length | 3 ft.
Connector Types | 4-Pin Mini DIN, Keyed; DB-9 Connectors

Related Products

The products related to the debug cable assembly are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
Dialogic® CSP 2090 Matrix Controller Series 3 Card | EXS-CPU-1300 | EXS-CPU-1300R

Debug Cable Assembly

The debug cable assembly is made up of the following components.

Pinouts

The debug cable assembly connector pinouts are listed below.

P1 Pinouts | Signal Name | DB-9
--- | --- | ---
1 | Receive (RCV) Data | 3
3 | Ground | 5
4 | Transmit (TX) Data | 2

The Matrix Controller Series 3 card is based on Motorola’s 750 PowerPC processor (68750). It is often referred to as the Matrix Controller.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.