0x2947 - SIP Request URI Header

Used in:
PPL Event Request message
PPL Event Indication message

Byte | Description
0, 1 | Tag 0x2947
2, 3 | Length Variable (maximum of 650 bytes)
4-n | Value[0-n]

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.