You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Disconnect Tone Pattern 0x001E

Disconnect Tone Pattern 0x001E

SwitchKit Name

DisconnectTonePattern

Type

EXS API and SwitchKit API message

Description

Disconnect Tone Pattern 0x001E

This message instructs the CSP to terminate call progress tone transmission on the specified channel.

Sent by

Host

SwitchKit Code

C Structure

typedef struct {

unsigned short Span;

UBYTE Channel;

} XL_DisconnectTonePattern;

C++ Class

class XLC_DisconnectTonePattern : public XLC_OneChannelOutbound {

public:

unsigned short getSpan() const;

void setSpan(unsigned short x);

UBYTE getChannel() const;

void setChannel(UBYTE x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x001E) | 3, 4 | Message Type (0x001E)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status (MSB, LSB)
Number of AEs to follow
AE 0x0D Channel
: | Checksum | 10 | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit