0x02C4 Gateway E164

This TLV contains the alias address which is added to the outbound H.323 setup message if the Outseize Control message or Route Control message does not contain the calling party number.
You can deconfigure the Gateway ID by setting this value to Null.

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x2C4 Gateway E164
2, 3 | Length Variable (maximum 32-byte ASCII character strings)
: | Value [n] 0-9, #, * Last character must be 0. Default is Null

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
ITU-T standard defines a set of call control, channel setup, and codec specifications for transmitting real-time voice and video over networks that do not offer guaranteed service or quality of service.
Outgoing call setup during real-time call processing on a specific channel.
A device that translates calls between an IP network and another network, typically the PSTN.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
American Standard Code for Information Interchange