You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > NGA Service Configure 0x0160

NGA Service Configure 0x0160

SwitchKit Name

NGAServiceConfigure

Type

NGA Service Configure 0x0160

EXS and SwitchKit API message

Description

Changes the service state for the M3UA object.

Sent by

Host application

Related API Messages

NGA Configure (0x0130)
NGA Configure Query (0x0131)
NGA Service Query (0x0161)
NGA State Notify (0x0163)
NGA State Query (0x0162)

SwitchKit Code

C Structure

typedef struct {

UBYTE AddrInfo[30];

UBYTE DataType;

UBYTE TLVCount;

UBYTE Data[221];

} XL_NGAServiceConfigure;

C Structure Response

typedef struct {

unsigned short Status;

UBYTE reserved6[13];

UBYTE AddrInfo[30];

UBYTE DataType;

UBYTE TLVCount;

UBYTE Data[219];

} XL_NGAServiceConfigureAck;

C++ Class

class XLC_NGAServiceConfigure : public XLC_OutboundMessage {

public:

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

void setAIBType(UBYTE x);

UBYTE getAIBType();

void setAECount(UBYTE x);

UBYTE getAECount();

void addAE(UBYTE AEpos, UBYTE AEtype, UBYTE AElen, UBYTE* AEvalue);

UBYTE* getAE(int AEpos);

void setAIBData(UBYTE* AIBDataPtr, UBYTE AIBDataLen);

UBYTE* getAIBData();

UBYTE getDataType() const;

void setDataType(UBYTE x);

UBYTE getTLVCount() const;

void setTLVCount(UBYTE x);

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

}

C++ Class Response

class XLC_NGAServiceConfigureAck : public

XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

const UBYTE *getAddrInfo() const;

UBYTE *getAddrInfo();

void setAddrInfo(UBYTE *x);

void setAIBType(UBYTE x);

UBYTE getAIBType();

void setAECount(UBYTE x);

UBYTE getAECount();

void addAE(UBYTE AEpos, UBYTE AEtype, UBYTE AElen, UBYTE* AEvalue);

UBYTE* getAE(int AEpos);

void setAIBData(UBYTE* AIBDataPtr, UBYTE AIBDataLen);

UBYTE* getAIBData();

; UBYTE getDataType() const;

void setDataType(UBYTE x);

UBYTE getTLVCount() const;

void setTLVCount(UBYTE x);

const UBYTE *getData();

UBYTE *getData();

void setData(UBYTE *x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0x00NN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x0160) | 3, 4 | Message Type (0x0160)
5, 6 | Sequence Number | 5, 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x03 - Item | 8 | Checksum
Number of AEs to Follow |  |
AEs 0x67 Functional Area 0x08 SS7 Stack 0x64 Global Object Type |  |
: | Data Type 0x00 - TLVs |  |
: | Number of TLVs |  |
: | 0xE001 Command |  |
: | Data TLV 0x9048 Application Server In Service |  |
: | Checksum |  |

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.