0x2794 Destination IP Address

Used in:
NPDI Universal ICB (0x0033) in:
Route Control message
Request for Service with Data message
Outseize Control message

Byte | Description
0, 1 | Tag 0x2794 Destination IP Address
2, 3 | Length 0x0004
4-7 | Value[0-3] IP Address

Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Outgoing call setup during real-time call processing on a specific channel.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).