0x9052 Route Set

Used in:
NGA Configure message

Byte | Description
0,1 | Tag 0x9052
2,3 | Length 0x0010
4-7 | Value[0-3] Destination Point Code
8,9 | Value[4,5] Number of Routes
10,11 | Value[6,7] Route ID
12,13 | Value[8,9] Signaling Gateway ID
14-17 | Value[10-13] Network Appearance
18,19 | Value [14,15] Priority

A number that addresses a node in a SS7 network.
A device that translates calls between an IP network and another network, typically the PSTN.