0x0008 IP Signaling Series 3 Card Compatibility Tag

Used in:
Matrix Configure message (0x7D)
IP Signaling Series 3 Card Query message (0x0101)
IP Signaling Series 3 Card Configure message (0x0100)

Byte | Description
0, 1 | Tag 0x0008
2, 3 | Length 0x0002
4 | Value[0] Value set up on both sides of the interface, MSB 0x00-0xFF
5 | Value[1] Value set on both sides of the interface, LSB 0x00 - 0xFF

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Most Significant Bit
Least Significant Bit