You are here: SwitchKit® Development Environment - CSA User’s Guide > 6 Configuring Resource Cards > Configuring DSP Alarm Thresholds

Configuring DSP Alarm Thresholds

This procedure describes how to configure the DSP alarm thresholds.

Before you begin

You must have a node view window open in configuration mode.

Steps to Configure DSP alarm thresholds

Do the following to configure DSP alarm thresholds:

Right-click the slot containing the DSP S2 card in the node view and select Configure Alarm Thresholds from the menu. The Configure DSP S2 Alarm Thresholds ... dialog box opens.

Change the values for the Number of Hits per Window, Window Size, and Threshold Value where required and then click OK.

The valid range of values for these fields are

Field | Range of Values
--- | ---
Number of Hits per Window | 1-16
Window Size | 1-16
Threshold Value | Variable. (microseconds or percentage)

Digital Signal Processor